Mechanical Engineering Department

Assignment

Of

Drawing Numbers

Locomotive, Shop & Miscel.

Drawing Numbers Assignment

1-4999 Locomotives & Miscel.

5000-5999 Locomotives (Old 8”x10”)

6000-7999 Locomotives (6” x 9”)

8000-8999 Som. Shop and Electric Locos.

30000-34999 Locomotives and Miscel.

35000-35399 H-3ka Locos.

35400- T-1-a Locos.

Passenger, Freight & Motor Cars

Drawing Numbers Assignment

10000-10999 Passenger Cars

20000-21659 “ “

21660-22999 Motor, Electric and Special Cars

23000-23434 Passenger Cars Built 1923

23435-24999 Passenger Cars

25000 Motor Rail Cars (Brill)

11000-14999 Freight Cars

15000-15059 “ “

Flats, Built 1924

15060-15499 Freight Cars

15500-15639 “ “

Hart Convt. 1924

15640-15799 Freight Cars Refrg. Built

1924

15800-19999 Freight Cars

Instructions

All cloth tracings are to have numbers assigned according to the above list.

Two index cards should be made out and filed; one in the corresponding group and one in numerical file.

No drawings which are made on vellum are to have numbers according to the above list. Such drawings are to have “A” sketch numbers and this number is to appear on the “Vellum” in the same location as that on a cloth tracing. All vellum drawings are to be made of standard sizes with border lines and the standard table in both of the right corners.

Incidentally, vellum drawings are to be made only for tentative work which is likely to be changed considerably before final completion or for small items which would probably not be used again.

All vellum drawings which are finally accepted must be traced on cloth; therefor, the small amount of extra time involved in making a cloth tracing of new work is considerably less than that spent in making a vellum and then a cloth tracing.

Harry A. Frye Collection, B&MRRHS

Transcribed 7-15-2019

FNN III